;
; Xinje USB driver setup information file
; Copyright (c) 2011 by Xinje Electric Co., Ltd. 
;
; This file supports:
;     Windows 2000
;     Windows XP,Vista,7
;
[Version]
Signature="$Windows NT$"
Provider=%MfgName%
DriverVer=03/09/2017,1.0.5.0

Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
CatalogFile=xnetusb.cat
[Manufacturer]
%MfgName%=DeviceList,NTamd64.5

[DeviceList]
%USB\VID_0471&PID_2400.DeviceDesc%=XnetUsbInstall.32, USB\VID_0471&PID_2400

[DeviceList.NTamd64.5]
%USB\VID_0471&PID_2400.DeviceDesc%=XnetUsbInstall.64, USB\VID_0471&PID_2400

[XnetUsbInstall.32.ntx86]
CopyFiles=XnetUsbCopyFiles
[XnetUsbInstall.64.NTamd64]
CopyFiles=XnetUsbCopyFiles.NTamd64

[XnetUsbInstall.32.ntx86.Services]
Addservice = XNETUSB, 0x00000002, XnetUsbAddService.32, XnetUsbInstallLog

[XnetUsbInstall.64.NTamd64.Services]
Addservice = XNETUSB, 0x00000002, XnetUsbAddService.64, XnetUsbInstallLog.64

[XnetUsbAddService.32]
DisplayName    = %XnetUsb.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 2                  ; SERVICE_AUTO_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\XnetUsb.sys
LoadOrderGroup = Base

[XnetUsbAddService.64]
DisplayName    = %XnetUsb.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 2                  ; SERVICE_AUTO_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\XnetUsb64.sys
LoadOrderGroup = Base

[XnetUsbInstallLog]
AddReg=XnetUsbInstallLogAddReg

[XnetUsbInstallLogAddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,XnetUsb.sys
;HKR,"XNETUSB\Parameters","MaximumTransferSize",0x10001,1023
;HKR,"XNETUSB\Parameters","DebugLevel",0x10001,2

[XnetUsbInstallLog.64]
AddReg=XnetUsbInstallLogAddReg.64

[XnetUsbInstallLogAddReg.64]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,XnetUsb64.sys
;HKR,"XNETUSB\Parameters","MaximumTransferSize",0x10001,1023
;HKR,"XNETUSB\Parameters","DebugLevel",0x10001,2

[XnetUsbCopyFiles]
XnetUsb.sys

[XnetUsbCopyFiles.NTamd64]
XnetUsb64.sys

[DestinationDirs]
DefaultDestDir = 10,System32\Drivers
XnetUsbCopyFiles = 10,System32\Drivers
XnetUsbCopyFiles.NTamd64      = 10,System32\Drivers

[SourceDisksNames]
1 = %XnetUsb.DiskName%,,0,

[SourceDisksFiles]
XnetUsb.sys = 1
XnetUsb64.sys = 1

;---------------------------------------------------------------;

[Strings]
MfgName = "Xinje Electric Co., Ltd."
USB\VID_0471&PID_2400.DeviceDesc="Xinje TH USB Device"
XnetUsb.SvcDesc="XnetUsb driver"
XnetUsb.DiskName="J-Link Installation Disk"


; *** EOF ***
